

***Mission Status Report 130***

***Reference Period: 01-15 Mar. 2023***

***Mission Status***

Overall

* The mission, in Phase E2 (Operations Phase) since 24th April 2018, has reached routine operations capacity at the beginning of March 2019.

Operational Products availability and access

* Level 1B Radiance/Irradiance, Level 2 Methane, Tropospheric Ozone (Offline); Aerosol Absorbing Index, Aerosol Layer Height, Carbon Monoxide, Cloud, Formaldehyde, Nitrogen Dioxide, Ozone Profile, Sulphur Dioxide, and Total Ozone products (Offline and Near Real Time) are available to the public via the Copernicus Sentinel-5 Precursor Data Hub – <https://s5phub.copernicus.eu>.

Platform

* Orbit Control Manoeuvre (OCM) activities were executed on 15th March between 17:27 – 18:12, with no noticeable impact on the quality of the data.

TROPOMI Payload

* The TROPOMI instrument continues measuring in nominal operations baseline with a 360 orbit repeat cycle and since 6th August 2019 with a spatial resolution of about 5.5 km along-track and 3.5 km across-track.

Ground Segment

* The status of both Flight Operations Segment (FOS) and Payload Data Ground Segment (PDGS) has been nominal. Routine scheduling, acquisition, processing and dissemination tasks were performed without major anomalies.
* An upgraded PDGS system was released on 15th March, including the implementation of updated KNMI processors to version 02.05.00.
* The full mission reprocessing of the Level 1B, Level 2 Sentinel-5P S-NPP Cloud information (auxiliary), Absorbing Aerosol Index, Aerosol Layer Height, Carbon Monoxide, Cloud, Methane, Nitrogen Dioxide and Total Ozone products was completed during end December 2022. The Sulphur Dioxide and Formaldehyde products reprocessing has been completed on 16th March. The Ozone Profile reprocessing is ongoing and foreseen to finish by the beginning of April. Due to some problems the Tropospheric Ozone reprocessing will be re-done (it takes less than one day).

Level 1B / Level 2 processors

* A new KNMI Ozone Profile processor was put into operations during the PDGS upgrade on 15th March. The aim is to significantly reduce the processing time by implementing the “checkerboard pattern” (e.g. only processing of half of the ground pixels) in the Near Real Time processing chain.

Cal/Val Activities

* The routine validation activities continued nominally for all products, including the reprocessed products.

PAL Activities

* Since 15th December 2021 a new Nitrogen Dioxide dataset reprocessed with the Sentinel-5P Product Algorithm Laboratory (PAL) using the official processor Version 2.3.1 is available to the users to allow consistent long-term data analysis (e.g., trends in air pollution based on COVID-19 impact). It covers the time period 1st May 2018 to 14th November 2021 and is available at <https://data-portal.s5p-pal.com>. It is now being replaced an upgraded product reprocessed with the PDGS. The reprocessed dataset is now available on the Data Hub – <https://s5phub.copernicus.eu>.
* Six pre-operational products (Aerosol Optical Thickness, Bromine Monoxide, Glyoxal, Sun-Induced Fluorescence, Water Vapour, and a Sulphur Dioxide product using the new Covariance-Based Retrieval Algorithm (COBRA)) are being provided to the public via <https://data-portal.s5p-pal.com>.

***Outlook***

* The reprocessed datasets for the Absorbing Aerosol Index, Carbon Monoxide, Cloud, and Total Ozone products were released to the public on 5th December 2022 and the Aerosol Layer Height, Methane, and Nitrogen Dioxide products were published during the first half of March. The publication of the reprocessed Level 1B product is ongoing and will be completed by the end of March. The missing reprocessed products (Sulphur Dioxide, Formaldehyde, Ozone Profile, and Tropospheric Ozone) will be publicly released by end April.
* The S5P Quality Working Group meeting will take place on 20th March, to discuss mainly on products algorithm evolution.

 *Report prepared by the ESA Sentinel-5 Precursor Team*